**Standard Operating Procedure**

**Plant Transporting Preparation**



**ODISHA MINING CORPORATION LTD.**

**KODINGAMALI BAUXITE MINE**

**Authorized By**

**Procedure:**

1. Only authorized personnel are allowed to work.
2. Ensure that all required PPE is in good condition and correctly fitted.
3. The plant must be towed, loaded and transported only in accordance with the operating instructions in the manual
4. For towing the plant, observe the prescribed transport position, admissible speed and itinerary.
5. Use only appropriate means of transport and lifting gear where applicable of adequate capacity.
6. The re-commissioning procedure must be strictly in accordance with the operating instructions in the manual
7. Before setting the plant in motion always check that the accessories have been safely stowed away.
8. When travelling on public roads, ways and places always observe the valid traffic regulations.
9. When crossing underpasses, bridges and tunnels or when passing under overhead lines always make sure that there is sufficient clearance.
10. Never travel across slopes, always keep the working equipment and the load close to the ground, especially when travelling downhill.